#!/usr/bin/python
# -*- coding: utf-8 -*-
#    
# Copyright (C) 2013, Arista Networks <netdevops@aristanetworks.com>
# 
# This program is free software: you can redistribute it and/or modify
# it under the terms of the GNU General Public License as published by
# the Free Software Foundation, either version 3 of the License, or
# (at your option) any later version.
#
# This program is distributed in the hope that it will be useful,
# but WITHOUT ANY WARRANTY; without even the implied warranty of
# MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
# GNU General Public License for more details.
#
# You should have received a copy of the GNU General Public License
# along with this program.  If not, see <http://www.gnu.org/licenses/>.
#
DOCUMENTATION = '''
---
module: arista_vlan
version_added: "1.3"
author: Peter Sprygada
short_description: Manage VLAN resources
requirements:
    - Arista EOS 4.10
    - Netdev extension for EOS
description:
    - Manage VLAN resources on Arista EOS network devices.  This module 
      requires the Netdev EOS extension to be installed in EOS.  For detailed
      instructions for installing and using the Netdev module please see 
      [link]
options:
    vlan_id:
        description:
            - the vlan id 
        required: true
    state:
        description:
            - describe the desired state of the vlan related to the config
        required: false
        default: 'present'
        choices: [ 'present', 'absent' ]
    logging:
        description:
            - enables or disables the syslog facility for this module
        required: false
        choices: [ 'true', 'false', 'yes', 'no' ]
    name:
        description:
            - a descriptive name for the vlan
        required: false
notes:
    - Requires EOS 4.10 or later 
    - The Netdev extension for EOS must be installed and active in the 
      available extensions (show extensions from the EOS CLI)
    - See http://eos.aristanetworks.com for details
'''

EXAMPLES = '''
Example playbook entries using the arista_vlan module to manage resource 
state.  
   
  tasks:
  - name: create vlan 999
    action: arista_vlan vlan_id=999 logging=true
    
  - name: create / edit vlan 999
    action: arista_vlan vlan_id=999 name=test logging=true
    
  - name: remove vlan 999
    action: arista_vlan vlan_id=999 state=absent logging=true
    
'''
import syslog
import json

class AristaVlan(object):
    """ This is the base class for managing VLAN resources in EOS network 
        devices.   This class provides basic CRUD functions for VLAN 
        resources.  This class acts as a wrapper around the netdev extension
        in EOS.  You must have the netdev extension installed in order for
        this module to work properly.   
        
        The following commands are implemented in this module:
            * netdev vlan create
            * netdev vlan list
            * netdev vlan show
            * netdev vlan edit
            * netdev vlan delete
    """
    
    attributes = ['name']

    def __init__(self, module):
        self.module     = module
        self.vlan_id    = module.params['vlan_id']
        self.name       = module.params['name']
        self.state      = module.params['state']
        self.logging    = module.boolean(module.params['logging'])
        
        
    @property
    def changed(self):
        """ The changed property provides a boolean response if the currently
            loaded resouces has changed from the resource running in EOS.
            
            Returns True if the object is not in sync 
            Returns False if the object is in sync.
        """
        return len(self.updates()) > 0
        
    def log(self, entry):
        """ This method is responsible for sending log messages to the local
            syslog.
        """
        if self.logging:
            syslog.openlog('ansible-%s' % os.path.basename(__file__))
            syslog.syslog(syslog.LOG_INFO, entry)
    
    def run_command(self, cmd):
        """ Calls the Ansible module run_command method.  This method will
            also send a message to syslog with the command name
        """        
        self.log("Command: %s" % cmd)
        return self.module.run_command(cmd.split())
        
        
    def delete(self):
        """ Deletes an existing VLAN resource from the current running 
            configuration.  A nonexistent VLAN will return successful for this
            operation.
            
            This method implements the following commands:
                * netdev vlan delete {vlan_id}
            
            Returns nothing if the delete was successful
            Returns error message if there was a problem deleting the vlan 
        """
        cmd = "netdev vlan delete %s" % self.vlan_id
        (rc, out, err) = self.run_command(cmd)
        resp = json.loads(out)
        if resp.get('status') != 200: 
            rc = resp['status']
            err = resp['message']
            out = None
        return (rc, out, err)
        
    def create(self):
        """ Creates a VLAN resource in the current running configuration.  If 
            the VLAN already exists, the function will return successfully.
            
            This function implements the following commands:
                * netdev vlan create {vlan_id} [--name <name>]
            
            Returns the VLAN resource if the create function was successful
            Returns an error message if there as a problem creating the vlan
        """
        attribs = []
        for attrib in self.attributes:
            if getattr(self, attrib):
                attribs.append("--%s" % attrib)
                attribs.append(getattr(self, attrib))
        
            cmd = "netdev vlan create %s " % self.vlan_id
            cmd += " ".join(attribs)
            
            (rc, out, err) = self.run_command(cmd)
            resp = json.loads(out)
            if resp.get('status') != 201:
                rc = int(resp['status'])
                err = resp['message']
                out = None
            else:
                out = resp['result']
        return (rc, out, err)
        
    def update(self):
        """ Updates an existing VLAN resource in the current running 
            configuration.   If the VLAN resource does not exist, this method
            will return an error.
            
            This method implements the following commands:
                * netdev vlan edit {vlan_id} [--name <name>]
            
            Returns an updated VLAN resoure if the create method was successful
        """
        attribs = list()        
        for attrib in self.updates():
            attribs.append("--%s" % attrib)
            attribs.append(getattr(self, attrib))
        
        if attribs:
            cmd = "netdev vlan edit %s " % self.vlan_id
            cmd += " ".join(attribs)
        
            (rc, out, err) = self.run_command(cmd)
            resp = json.loads(out)
            if resp.get('status') != 200:
                rc = int(resp['status'])
                err = resp['message']
                out = None
            else:
                out = resp['result']
            return (rc, out, err)
          
        return (0, None, "No attributes have been modified")
    
    def updates(self):
        """ This method will check the current VLAN resource in the running
            configuration and return a list of attributes that are not in sync
            with the current resource from the running configuration.
        """
        obj = self.get()
        update = lambda a, z: a != z
        
        updates = list()
        for attrib in self.attributes:
            value = getattr(self, attrib)
            if update(obj[attrib], update) and value is not None:
                updates.append(attrib)
        self.log("updates: %s" % updates)
        return updates
        
    def exists(self):
        """ Returns True if the current VLAN resource exists and returns False
            if it does not.   This method only checks for the existence of the
            VLAN ID.
        """
        (rc, out, err) = self.run_command("netdev vlan list")
        collection = json.loads(out)
        return str(self.vlan_id) in collection.get('result')
        
    def get(self):
        """ This method will return a dictionary with the attributes of the
            VLAN resource identified in vlan_id.   The VLAN resource has the 
            following stucture:
            
              {
                "vlan_id": <vlan_id>,
                "name": <name>
              }
            
            If the VLAN ID specified by vlan_id does not exist in the system, 
            this method will return None
        """
        cmd = "netdev vlan show %s" % self.vlan_id
        (rc, out, err) = self.run_command(cmd)
        obj = json.loads(out)
        if obj.get('status') != 200: 
            return None
        return obj['result']
        
        

def main():

    module = AnsibleModule(
        argument_spec = dict(
            vlan_id=dict(default=None, required=True, type='int'),
            name=dict(default=None, type='str'),
            state=dict(default='present', choices=['present', 'absent']),
            logging=dict(default=False, type='bool')
        ),
        supports_check_mode = True
    )
    
    obj = AristaVlan(module)
    
    rc = None
    result = dict()
    
    if obj.state == 'absent':
        if obj.exists():
            if module.check_mode: 
                module.exit_json(changed=True)
            (rc, out, err) = obj.delete()
            if rc !=0: 
                module.fail_json(msg=err, rc=rc)                
            
    elif obj.state == 'present':
        if not obj.exists():
            if module.check_mode: 
                module.exit_json(changed=True)
            (rc, out, err) = obj.create()
            result['results'] = out
        else:
            if obj.changed:
                if module.check_mode: 
                    module.exit_json(changed=obj.changed)
                (rc, out, err) = obj.update()
                result['results'] = out
            
        if rc is not None and rc != 0:
            module.fail_json(msg=err, rc=rc)
    
    if rc is None:
        result['changed'] = False
    else:
        result['changed'] = True
    
    module.exit_json(**result)
    

# import module snippets
from ansible.module_utils.basic import *
main()
